Software dependencies:

-At first you need to setup serial interface

$sudo raspi-config #-  interfacing - Serial ----enable it

$sudo apt install python3-requests

-Secondly place qr.py in home/pi

-Third to run the code: open terminal and push $sudo python qr.py

Hardware dependences:

1. Raspberry pi zero
2. RG LED
3. 2 330 ohm resistors
4. 3.3volt buzzer
5. 3.3volt relay

Schematic:



